This page is a snapshot from the LWG issues list, see the Library Active Issues List for more information and the meaning of C++17 status.

### 2441. Exact-width atomic typedefs should be provided

Section: 33.5.8 [atomics.types.generic] Status: C++17 Submitter: Stephan T. Lavavej Opened: 2014-10-01 Last modified: 2017-07-30

Priority: 0

View all other issues in [atomics.types.generic].

View all issues with C++17 status.

Discussion:

`<atomic>` doesn't provide counterparts for `<inttypes.h>`'s most useful typedefs, possibly because they're quasi-optional. We can easily fix this.

[2014-11, Urbana]

Typedefs were transitional compatibility hack. Should use `_Atomic` macro or template. E.g. `_Atomic(int8_t)`. BUT `_Atomic` disappeared!

Detlef will look for `_Atomic` macro. If missing, will open issue.

[2014-11-25, Hans comments]

There is no `_Atomic` in C++. This is related to the much more general unanswered question of whether C++17 should reference C11, C99, or neither.

[2015-02 Cologne]

AM: I think this is still an SG1 issue; they need to deal with it before we do.

[2015-05 Lenexa, SG1 response]

Move to SG1-OK status. This seems like an easy short-term fix. We probably need a paper on C/C++ atomics compatibility to deal with `_Atomic`, but that's a separable issue.

[2015-10 pre-Kona]

SG1 hands this over to LWG for wording review

Proposed resolution:

This wording is relative to N3936.

1. Change 33.5.8 [atomics.types.generic] p8 as depicted:

   > -8- There shall be atomic typedefs corresponding to the typedefs in the header `<inttypes.h>` as specified in Table 147. `atomic_intN_t`, `atomic_uintN_t`, `atomic_intptr_t`, and `atomic_uintptr_t` shall be defined if and only if `intN_t`, `uintN_t`, `intptr_t`, and `uintptr_t` are defined, respectively.

2. Change 99 [atomics.types.operations.req], Table 147 ("`atomic` `<inttypes.h>` typedefs"), as depicted:

   > Table 147 — `atomic` `<inttypes.h>` typedefs
   > Atomic typedef | `<inttypes.h>` type
   > --- | ---
   > `atomic_int8_t` | `int8_t`
   > `atomic_uint8_t` | `uint8_t`
   > `atomic_int16_t` | `int16_t`
   > `atomic_uint16_t` | `uint16_t`
   > `atomic_int32_t` | `int32_t`
   > `atomic_uint32_t` | `uint32_t`
   > `atomic_int64_t` | `int64_t`
   > `atomic_uint64_t` | `uint64_t`
   > `…`